|  |  |
| --- | --- |
|  | **Epoxychic**.com **907 322 6295**   Moosepath LLC General Contractor #2101218985 1127 Cass Road, Traverse City MI |

**Contract**

|  |  |
| --- | --- |
| **Item** | **Cost** |
| Estimate |  |
| Site visit |  |
| Custom sample if existing samples are inadequate |  |
| Additional samples (allow 7-10 business days) |  |
| Repair existing surface (e.g. level, patch, sand, etc.) |  |
| Sink removal and installation (we are not licensed plumbers and you may wish to hire one) |  |
| Other: |  |
| **Total** |  |
| **Deposit (Due on signing)** |  |
| **Remainder (Due on day of completion)** |  |

1. We will attempt to minimize imperfections and level customer-provided surfaces but cannot guarantee perfection.
2. Each surface is a unique and custom piece and you should expect slight variations. We believe this is a benefit to your artisan crafted masterpiece. No two are ever alike.
3. While we cannot promise an exact duplication of pictures and samples, we will attempt to get as close to your desired look as possible. By agreeing to this contract, you acknowledge that you trust the craftsman to make the best decision for your space; sometimes adjusting without need for consent.
4. The machine produced, smooth edge you may find with other mass-produced products are not likely with handcrafted countertops as all overlay edges are created by hand and have natural variations.
5. Minor imperfections (small depressions, slight ripples, dust particles, etc.) can occur with the hand applied epoxy layer. If they occur, the imperfections may or may not be able to be corrected. You can assist in preventing these issues by minimizing human and pet traffic and reducing air movement caused by fans and heating/cooling systems.

Any countertop material can be scratched with normal use. Epoxy is 7/8 on the hardness scale and compares to Corian. Using other products harder than epoxy can scratch the surface, such as porcelain, Fiesta ware, etc. Do not pull items across your countertop surface and avoid abrasive cleaners. Use cutting boards. Water and mild detergents are generally all that is needed to keep your countertop clean. Scratches in epoxy may be repairable.

1. Note that epoxy cures over about 30 days. Curing time varies with air temperature, humidity, and other factors. While the countertop is usable during this curing period, take extra care to avoid scratching your new countertop. Limit the placement of heavy appliances on the countertop for 30 days and use pads under heavy items.
2. A two-year warranty covers defects of delamination or color fade ONLY. Cuts, chips, scratches and/or other damage caused to the overlay are not grounds for warranty.

I have read and understood all statements listed above and agree to have Moosepath LLC perform the overlay process on my surfaces.

Acknowledged By: Date:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_