|  |  |
| --- | --- |
|  | **Epoxychic**.com **907 322 6295**   Moosepath LLC General Contractor #2101218985 1127 Cass Road, Traverse City MI |

**Tips for you**

# Before the process

* Clean. clean. clean. The less dust in your house the better your counter tops will turn out.
* Remove the sink before we arrive to your house unless we are removing ii for you.
* Our charge for sink an installs and removals is S150 per sink.
* Please note that we are not licensed plumbers. If you buy a new sink. your drains must match up.
* Your countertop has a warranty against delamination. It does not cover damage done by the customer such as dents. and scratches.
* Scratches can be removed with rubbing compound or paste wax. You can wax your counter tops every couple of months to protect them from wear and tear.

# After the process:

* Wait 30 days to put anything hot on tile epoxy as it takes 30 days for a full cure. After curing, you may put anything on it up to 500f. Do not place items with sustained heat on the surface (e.g. a crock pot).
* You may put your sink and appliances back in place after a full day of cure and around 3 days after the countertop work. Use caution when replacing appliances as new epoxy is still malleable.
* Wait five days before putting items such as a coffee maker, knife rack, etc. as heavy objects can leave dents before the epoxy hardens.
* Resist the urge to check up on your counter during the first six hours. Dust and hair can easily end up in the epoxy.
* Keep animals in other rooms.